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Angel Pocket Sewing Instructions

Items Needed:

white Treaa
2piaces ofwhita satinibbon (8 inches ong 14 nch wide)
3 squarepieces ot whitafabric

+squara pice of whits lace fabric

Sowing Machine

susigntPins

Scissors

Steam ran or snd ron and e

‘Step #1: Cutting (I pieces are already cut, skip this step)

Using either an 8 or 10inch quilters square, cut out three square pieces on white fabric and one square
piece from white lace. Cut two pieces 8 inch n length of white satinribbon.

Step #2: Ironing

ron all pieces to make sure they are flat. After all pieces are roned, take one piece, and fold itin ke a.
triangte, with the correct side of the fabric out, and ron the fold flat. The triangle piece willbe the pocket.
Whenyouare finished should have four fabric pieces like this:
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: Sow Pocket Top Stitch

Take the triangle pocket piece, using % n seam allowance, sew atop stitch along the long edge of the

‘Step #4: Stacking and Pinning Fabric to Sew

Take one piece of whits fabric and lay it flat on the table like a diamond., Next place the lace piece ight
side up on top of the white piece i the same position. Next place the triangle piece on top of the lace.
piece with point of the triangle matching at the bottom points of the diamond and the sttching across
the middle.
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Step #5: Place Ribbon

Take one piece ofribbon and place the edge of the ribbon in the left comer of the diamond undereath
thefold triangle piece running parallel with the fld.

Take the second piece of ibbon and place the edge of the ibbon n the left coer of the diamond
running undemeatn the fold triangle piece running parallel with the fold.

Ribbon here Ribbon here

Note: the ibbons may overlap in the middle. Thatis fine.

Step 6: Place Final Square Fabric and Pin

Take the remaining square piece of fabric with rght side down, place on the back of the diamond
matching al four cormer and pin everything together. Make sure that the edges of the ribbon in the
‘corners ar held by a pin because they will sip during sewing.

OO

Using a inch seam allowance, sew around the entire square leaving a two-inch opening on one side to
allow the packet to be tumed right-side out.

Step7: Sewing

5> 2inch opening

‘Step 8: Turn Right-Side out and Iron

After sewing, trim the corners (but do not trim the seams) make sure that all pins are removed and turn
the packet right.side out. A pin may be needed to assist in pulling the comers to the diamond shape.
Pullon the ribbons if needed to help make the diamond shape again. The lace piece should be on the
‘opposite side of the pouch. If needed, use pins to help keep fabric in place for the next step.

Step 9: Topstitch

Make sure that the ribbons are pulled out from the pocket and laying straight out. Using a % nch seam
allowance, topstitch the pocket making sure that the fabric at the hole s tucked in and closed.

Ribbo Ribbo

At the topstitchis complete, trim off any loose threads and remove all pins. Tie the ribbon togsther on
the side of the pouch and the project s complete.
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